Imaging configuration created for ARLON_DPF_4560GT
Roland DGA VersaCAMM VP-540
Wasatch SoftRIP 6.2

720x720-dpi
16-pass @ 750mm/sec
bi-directional printing
Heater settings: print=38C/100F  dryer=50C/122F
